**BJT P.3**

Design the bias circuit (find values of RC and RB) for the figure below to give a Q-point of IC = 20µA and VCE = 0.9V if the transistor current gain βF = 50 and VBE = 0.65V. What is the Q-point if the current gain of the transistor is actually 125?

